; WARNING:  It is not recommended for end users to manipulate this file unless
;           instructed to do so by a Teklynx technical support representative.  
;           Be sure to make a backup copy before making any changes.
;
; Format:
;    The [Manufacturers] section consists of the manufacturer name followed by
;    a T for Teklynx drivers, an S for StrandWare drivers or a V for LabelView
;    drivers, all separated by semicolons.
;
;    Each entry under the manufacturer's section includes the DLL name to use,
;    the selection name of the printer model, the code for the type of driver
;    it is (also T, S, or V), the internal name, the id number, the Windows NT
;    DLL name for the generic Windows driver, and the Windows 95 driver name
;    for the generic Windows printer.  The last parameter may be omitted.
;
;
; The next Teklynx printer ID to use is 4189.
;
;  Log of changes made to this file
;
;  20040701 WLG Created initial file for TSC OEM
;
;

[Version]
; Do not change this field
Ver=3

; This field should be incremented each time modifications are made
revision=4

[Manufacturers]
1=Barcode Printer;V


[Barcode Printer] 
1=Dummy.dll;Deluxe 200;V;DELUXE_200;659;Teklynx1.dll;TSC.DRV
2=Dummy.dll;Deluxe 200M;V;DELUXE_200M;864;Teklynx1.dll;TSC.DRV
3=Dummy.dll;Deluxe 300;V;DELUXE_300;660;Teklynx1.dll;TSC.DRV
4=Dummy.dll;Deluxe 300M;V;DELUXE_300M;865;Teklynx1.dll;TSC.DRV
5=Dummy.dll;Action 200;V;ACTION_200;866;Teklynx1.dll;TSC.DRV
6=Dummy.dll;Action 200 Plus;V;ACTION_200PLUS;867;Teklynx1.dll;TSC.DRV
7=Dummy.dll;TT024-50;V;TT024_50;868;Teklynx1.dll;TSC.DRV
8=Dummy.dll;DT024-50;V;DT024_50;869;Teklynx1.dll;TSC.DRV
9=Dummy.dll;TT024-60;V;TT024_60;870;Teklynx1.dll;TSC.DRV
10=Dummy.dll;T-462;V;T_462;871;Teklynx1.dll;TSC.DRV
11=Dummy.dll;T-443;V;T_443;872;Teklynx1.dll;TSC.DRV
12=Dummy.dll;T-0612;V;T_0612;873;Teklynx1.dll;TSC.DRV

[Synonyms]
